
https://jlcpcb.com/
JLCPCB

==========
JLCPCB ('QUICK TURN PCB 7 LAYERS ONLY') COMPATIBLE INFO

==========
PCB EDITOR GERBER/DRILL FILES EXPORT
EXTENSION RENAME:
KICAD_GBR --> EDIT_GBR
1. Board Outline *-Edge_Cuts.gbr --> *-EDGE.GKO
2. Plated Drills *-PTH.drl --> *-DRILL1.XLN (EXCELLON FORMAT)
2. Non-Plated Drills *-NPTH.drl --> *-DRILL2.XLN
3. Top SilkScreen *-F_Silkscreen.gbr --> *-SSTOP.GTO
4. Top SolderMask *-F_Mask.gbr --> *-SMTOP.GTS
5. Top Copper *-F_Cu.gbr --> *-CPRTOP.GTL
6. Bottom Copper *-B_Cu.gbr --> *-CPRBTM.GBL
7. Bottom SolderMask *-B_Mask.gbr --> *-SMBTM.GBS

.XLN  (EXCELLON FORMAT)
==========

==========
EXAMPLES:
[ProjectName]_1-EDGE.GKO
[ProjectName]_2-DRILL1.XLN
[ProjectName]_3-SSTOP.GTO
[ProjectName]_4-SMTOP.GTS
[ProjectName]_5-CPRTOP.GTL
[ProjectName]_6-CPRBTM.GBL
[ProjectName]_7-SMBTM.GBS
(Optional)
[ProjectName]-DRILL2.XLN
==========

==========
IMPORTANT EDIT!
REMOVE THE FOLLOWING FROM ALL GERBER FILES (NEAR TOP):

%TF.GenerationSoftware,KiCad,Pcbnew,8.0.3*%
%TF.CreationDate,2024-09-14T22:30:49-07:00*%
%TF.ProjectId,AUDIOMXR,41554449-4f4d-4585-922e-6b696361645f,rev?*%
%TF.SameCoordinates,Original*%
%TF.FileFunction,Copper,L2,Bot*%
%TF.FilePolarity,Positive*%

G04 Gerber Fmt 4.5, Leading zero omitted, Abs format (unit mm)*
G04 Created by KiCad (PCBNEW 8.0.3) date 2024-09-14 22:30:49*

 ----------
TOP OF FILE SHOULD CONTAIN ONLY:
%FSLAX45Y45*%
%MOMM*%
----------

REMOVE THE FOLLOWING FROM ALL DRILL FILES (NEAR TOP):
; DRILL file {KiCad 8.0.3} date 2024-09-14T22:30:21-0700
; FORMAT={-:-/ absolute / inch / decimal}
; #@! TF.CreationDate,2024-09-14T22:30:21-07:00
; #@! TF.GenerationSoftware,Kicad,Pcbnew,8.0.3
; #@! TF.FileFunction,Plated,1,2,PTH
FMAT,2
INCH
==========

==========
KICASD GERBER VIEWER IMPORT FOR EXPORT TO PCB EDITOR:

Open ZIP File [ProjectName]_GRBR.zip ...
Export to PCB Editor ...
Filename: [ProjectName].kicad_pcb

Layer Selection:
[ProjectName]_CopperBottom --> B.Cu
[ProjectName]_CopperTop --? F.Cu (OPTIONAL)
*[ProjectName]_DrillHoles --> Hole Data (DO NOT EXPORT)
[ProjectName]_SilkScreenTop --> F.SilkS
[ProjectName]_SolderMaskBottom --> B.Mask
[ProjectName]_SolderMaskTop --> F.Mask
[ProjectName]_BoardOutline --> Edge Cuts

*(Export as Separate Reference File
Filename: [ProjectName_Drill].kicad_pcb)
==========
